REM \*\*\* CONVERT DUAL SETPOINT TO SINGLE SETPOINT \*\*\*

REM ----- 12-05-16 ---- GS -- Models BAC-90XX

REM Use AV5 as Setpoint Reference When Occupied Mode is Active

REM Changes need to be made in the Netsensor configuration under "User Setpoints" tab

REM to reflect that AV5 is the only point Manipulated for Setpoint control

IF MSV1 = 3 AND BV4 = 0 THEN END

IF MSV1 = 1 OR BV4 = 1 THEN AV3@8 = AV5 + AV11 / 2 , AV4@8 = AV5 - AV11 / 2

IF MSV1 = 2 THEN AV3@8 = AV5 + AV12 , AV4@8 = AV5 - AV12

END